{"text_format":"2","workbook":"xls","n_sheets":2,"sheets":["睢县职教中心汽修专业需购设备清单","AHK毕业考试1工具材料准备清单"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"睢县职教中心汽修专业需购设备清单","index":0,"n_rows":162,"n_cols":7,"rows_kept":162,"cut":false,"hidden":false,"merged":[[0,0,0,6],[1,0,1,6]],"flags":["formulas_cached_only"]}
["第一标段设备清单1"]
["1、睢县职教中心汽修专业需购设备清单"]
["序号","名称","技术参数","单位","数量","单价","合计"]
[1,"离合器、传动轴、驱动桥","大众系列8成翻新离合器、传动轴、驱动桥","套",1]
[2,"* 气压制动系统实训台","*提供原厂授权和售后服务承诺","台",1]
[3,"* 动力转向及悬架实训台","*提供原厂授权和售后服务承诺","台",1]
[4,"电控汽油发动机总成散件","","台",4]
[5,"电控汽油发动机拆装翻转架","","台",4]
[6,"汽车故障电脑诊断仪","","台",1]
[7,"空调清洗机","","台",1]
[8,"* 汽车空调诊断仪","*提供原厂授权和售后服务承诺","台",1]
[9,"* 制冷剂鉴别仪","*提供原厂授权和售后服务承诺","台",1]
[10,"风速计","","台",1]
[11,"* 车轮定位仪","*提供原厂授权和售后服务承诺","台",1]
[12,"* 剪式举升机","*提供原厂授权和售后服务承诺","台",1]
[13,"* 底盘系统综合实训台","*提供原厂授权和售后服务承诺","台",1]
[14,"* 外形修复机","*提供原厂授权和售后服务承诺","台",1]
[15,"等离子切割机","","台",1]
[16,"双向钣喷架","·整体焊接式，固定于地面，结构牢固。\n·多功能性，可同时使用多种不同规格类型汽车\n·前翼子板、车门、等放置作业；\n·人性化设计，操作、安装方便快。外形美观新颖，结构合理，方便维护`\n·规格尺寸 ：1140X900X600MM","台",4]
[17,"电动钣金除漆除锈机","·转速：12000转/分钟    \n·工作压力：6～7巴\n·净重：1.2Kg    \n·进气口径：1/4\"   轴心公螺：M10×1.5\n·适用于钣金旧漆、铁锈刷除，不伤钣金表面\n·配4\"砂碟或可选配黑金钢研磨轮φ16","台",1]
[18,"气动钣金切割锯","技术参数：\n1.砂器座尺寸：锯片24T，32齿\n2.耗 气 量：0.4m3/min\n3.管 尺 寸：5×8mm\n4.进气口连接：1/4″\n5.自由转速：10000R.P.M\n使用压力：6.5kg","台",1]
[19,"气动钣金牵引器","·专用于大面积汽车钣金凹陷变形的整形\n·滑动锤重量：1.5Kg\n·总长度：1120mm       \n· 净重：3.355Kg\n·工作压力：6巴             \n·进气口径：1/4\"\n·配两个吸盘：φ120mm、φ155mm","台",1]
[20,"气动打磨机","功能特点：\n1.转    速：3600 转/分钟\n2.进气口径：1/4\"\n3.气    压：6巴\n4.耗 气 量：132升/分钟\n配3\"和5\"尼龙搭扣盘、3\"和5\"无孔砂纸各5张。","个",2]
[21,"气动焊点削钻机","·专业钻除汽车钣金焊点，有防滑底托装置\n·转速：1800转/分钟   耗气量：283升/分钟\n·套装含：4支钻咀、1个油雾器、1个开紧匙、1个接头","台",1]
[22,"汽车挡风玻璃切除机","专用于切割固化后玻璃胶，尤其适合各种车挡风玻璃的拆卸 拆卸快速，更安全","个",2]
[23,"龙神缝隙手磨器","质地柔软，握拿方便主要用于对机械工具无法研磨的小区域进行修复。\n粘上砂纸即可手动研磨。 \n长度：100mm 用于缝隙打磨","块",5]
[24,"洗枪小号刷子","用于清洗喷枪枪身及零部件","把",10]
[25," 路贝狮无尘干磨设备","技术参数：\n功率：2*1000瓦（双马达）\n输入气压：6公斤\n最大耗气量：1450 升/分钟\n集尘量：220-260立方米/小时\n集尘袋容量：7公斤\n噪音：72分贝\n自重：26公斤\n可同时接两把电动或两把气动磨灰机\n","套",1]
[26,"RH153A 干磨机","手掌式细磨磨灰机，偏心3mm","台",2]
[27,"RH156A 干磨机","手掌式细磨磨灰机，偏心6mm","台",2]
[28,"RH159A 干磨机","手掌式细磨磨灰机，偏心9mm","台",1]
[29,"PPGPlus干磨搭扣式手刨 "," 70*125mm ","个",1]
[30,"PPGPlus干磨搭扣式手刨 "," 70*198mm ","个",1]
[31,"PPG干磨砂纸P80","70*198，50张/盒","盒",1]
[32,"PPG干磨砂纸P120","70*198，50张/盒","盒",1]
[33,"PPG干磨砂纸P180","70*198，50张/盒","盒",1]
[34,"PPG干磨砂纸P240","70*198，50张/盒","盒",1]
[35,"PPG干磨砂纸P320","70*198，50张/盒","盒",1]
[36,"PPG干磨砂纸P400","70*198，50张/盒","盒",1]
[37,"PPG干磨砂纸P80","6寸15孔，50张/盒","盒",1]
[38,"PPG干磨砂纸P120","6寸15孔，50张/盒","盒",1]
[39,"PPG干磨砂纸P180","6寸15孔，50张/盒","盒",1]
[40,"PPG干磨砂纸P240","6寸15孔，50张/盒","盒",1]
[41,"PPG干磨砂纸P320","6寸15孔 ，50张/盒","盒",1]
[42,"PPG干磨砂纸P400","6寸15孔，50张/盒","盒",1]
[43,"PPG干磨砂纸P500","6寸15孔，50张/盒","盒",1]
[44,"PPG菜瓜布GP 320","20片/盒","盒",1]
[45,"PPG菜瓜布VF 360","20片/盒","盒",1]
[46,"PPG菜瓜布UF 1500 ","20片/盒","盒",1]
[47,"PPG菜瓜布MF 2000 ","F02095,20片/盒","盒",1]
[48,"PPG菜瓜布MF 2500 ","3340-F02096,20片/盒","盒",1]
[49,"PPG海绵干磨软垫  ","145mm 6+8+1孔，5片/包","片",1]
[50,"PPG保护垫 ","145mm 49孔 ，5片/包","片",1]
[51,"PPG保护垫 ","70*198mm 22孔，5片/包","片",1]
[52,"遮蔽膜  ","15mm*400mm*20m 60卷/箱","件",1]
[53,"遮蔽膜 ","18mm*1500mm*20m 25卷/箱 ","件",1]
[54,"皱纸胶带 ","18mm-50m，3520-1850","箱",1]
[55,"打磨指剂套装","手柄+碳粉30克，3510-0180","套",1]
[56,"打磨指示剂 ","碳粉30克 3510-0181","盒",1]
[57,"洗手膏"," H65116P15盎司","罐",1]
[58,"洗手膏","60盎司 H65217P","罐",1]
[59,"防静电工作服 ","3520-3002","件",1]
[60,"PPG除尘布","6060-1201","盒",1]
[61,"原子灰搅拌板","3510-0007","个",1]
[62,"PPG Plus 免洗枪壶套装 ","3510-0117","套",1]
[63,"PPG纸漏斗","3510-0301","箱",1]
[64,"PPGPlus防尘口罩","一次性防尘口罩","盒",1]
[65,"PPGPlus水性研磨膏 ","700G/支","支",1]
[66,"PPG喷漆量杯","测量油漆容量","个",1]
[67,"大卷式除油布","（500片/卷） 3510-0779","卷",1]
[68,"PPGPlus干磨搭扣式手刨 ","70*125mm","个",1]
[69,"PPGPlus干磨搭扣式手刨 ","70*198mm ","个",1]
[70,"905泥黄","2.5L/桶","桶",1]
[71,"907铁黄","2.5L/桶","桶",1]
[72,"920紫色","2.5L/桶","桶",1]
[73,"933蓝黑","2.5L/桶","桶",1]
[74,"952坚蓝","2.5L/桶","桶",1]
[75,"978绯色","1L/桶","桶",1]
[76,"938银底控色剂","1L/桶","桶",1]
[77,"942铁红","1L/桶","桶",1]
[78,"975青铜","1L/桶","桶",1]
[79,"982铁黄","1L/桶","桶",1]
[80,"983深黄","1L/桶","桶",1]
[81,"926超级红","2.5L/桶","桶",1]
[82,"930发红蓝","2.5L/桶","桶",1]
[83,"902通白","1L/桶","桶",1]
[84,"903中淡黄","1L/桶","桶",1]
[85,"904通黑","1L/桶","桶",1]
[86,"908赤褐","1L/桶","桶",1]
[87,"96酒红","1L/桶","桶",1]
[88,"910深蓝","1L/桶","桶",1]
[89,"900超级纯白","2.5L/桶","桶",1]
[90,"919青紫","1L/桶","桶",1]
[91,"921通红","1L/桶","桶",1]
[92,"922湖蓝","1L/桶","桶",1]
[93,"941深红","2.5L/桶","桶",1]
[94,"948黑色","1L/桶","桶",1]
[95,"950深黑","1L/桶","桶",1]
[96,"954蓝青","1L/桶","桶",1]
[97,"956超级蓝","1L/桶","桶",1]
[98,"957坚蓝","1L/桶","桶",1]
[99,"971光红","1L/桶","桶",1]
[100,"917高浓绿金","1L/桶","桶",1]
[101,"923光褐红","1L/桶","桶",1]
[102,"937淡黄","1L/桶","桶",1]
[103,"961洋红","1L/桶","桶",1]
[104,"967深邃黑","1L/桶","桶",1]
[105,"972琥珀黄","1L/桶","桶",1]
[106,"973亮橙","1L/桶","桶",1]
[107,"976紫红","1L/桶","桶",1]
[108,"980艳红","1L/桶","桶",1]
[109,"985幼银","1L/桶","桶",1]
[110,"984中闪银","1L/桶","桶",1]
[111,"986中银","2.5L/桶","桶",1]
[112,"987中粗银","2.5L/桶","桶",1]
[113,"988粗银","1L/桶","桶",1]
[114,"989特粗银","1L/桶","桶",1]
[115,"991丝绸银","1L/桶","桶",1]
[116,"992特闪粗银","1L/桶","桶",1]
[117,"998元宝粗银","1L/桶","桶",1]
[118,"CS32梦幻紫","0.33L/桶","桶",1]
[119,"CS33激光红","0.33L/桶","桶",1]
[120,"CS34热力橙","0.33L/桶","桶",1]
[121,"3762K调和清漆","2.5L/桶","桶",1]
[122,"5600银底色控色剂","2.5L/桶","桶",1]
[123,"528高银底色控色剂","2.5L/桶","桶",1]
[124,"475纯色底控色剂","1L/桶","桶",1]
[125,"6850清漆","5L/桶","桶",1]
[126,"6060清漆","5L/桶","桶",1]
[127,"588+760标准清漆+固化剂","5L+2.5L","桶",1]
[128,"790超快干固化剂","2.5L/桶","桶",1]
[129,"938高浓度固化剂（低气温）","2.5L/桶","桶",1]
[130,"939高浓度固化剂（高气温）","2.5L/桶","桶",1]
[131,"510高固含量厚膜底漆（灰色）","3.5L/桶","桶",1]
[132,"511高固含量厚膜底漆（白色）","3.5L/桶","桶",1]
[133,"9850无硌侵蚀底漆","1L/桶","桶",1]
[134,"895快干无硌环氧底漆","1L/桶","桶",1]
[135,"5670 高固含量底漆色母","0.5L/桶","桶",1]
[136,"5000紫外光速干底漆","0.5L/桶","桶",1]
[137,"5605自流平底漆灰色","2.5L/桶","桶",1]
[138,"5601自流平底漆深灰色","1L/桶","桶",1]
[139,"1086防走珠水","1L/桶","桶",1]
[140,"14除油剂","5L/桶","桶",1]
[141,"1402除油剂","（高温)，5L/桶","桶",1]
[142,"1050原子灰","2L/桶","桶",1]
[143,"1052万能原子灰","2L/桶","桶",1]
[144,"1057纤维原子灰","1.8L/桶","桶",1]
[145,"007全能合金灰","3.8L/桶","桶",1]
[146,"A242快干填眼灰","200ml/桶","桶",1]
[147,"2020柔软添加剂","0.5L/桶","桶",1]
[148,"1050防静电清洁剂","1L/桶","桶",1]
[149,"2001单组份塑料底漆","1L/桶","桶",1]
[150,"1401驳口水","1L/桶","桶",1]
[151,"1491低气温稀释剂","5L/桶","桶",1]
[152,"1492标准气温稀释剂","5L/桶","桶",1]
[153,"1493高气温稀释剂","5L/桶","桶",1]
[154,"1494极炎热气温稀释剂","5L/桶","桶",1]
[155,"1692--2K双组份低VOC稀释剂","快干，5L/桶","桶",1]
[156,"1693--2K双组份低VOC稀释剂 ","中干，5L/桶","桶",1]
[157,"1694--2K双组份低VOC稀释剂 ","慢干，5L/桶","桶",1]
[158,"1689-2K高固含量稀释剂","2.5L/桶","桶",1]
[159,"* 钣金技术构造与维修资源库"," *提供原厂授权和售后服务承诺","套",1]

{"sheet":"AHK毕业考试1工具材料准备清单","index":1,"n_rows":127,"n_cols":6,"rows_kept":127,"cut":false,"hidden":false,"merged":[[0,0,0,5],[1,0,1,5]],"flags":["formulas_cached_only"]}
["第一标段设备清单2"]
["2、项目学校13级AHK毕业考试1工具材料准备清单"]
["序号","名称","规格","数量/每学生","共需","备注"]
[1,"塑料PVC","40x30x25","根",14,"40mm*30mm*25mm"]
[2,"铝板","  60 x 30 x 1mm","张",14,"60mm*30mm*1mm"]
[3,"手用丝锥","M4","只",14,"M4"]
[4,"手用丝锥","M5","只",14,"M5"]
[5,"铰杠","160mm","根",7,"钳工专用160mm"]
[6,"锯条","300mm","根",100,"300mm"]
[7,"麻花钻",3.3,"根",14,"Φ3.3"]
[8,"麻花钻",4.5,"根",14,"Φ4.5"]
[9,"麻花钻",5.5,"根",14,"Φ5.5"]
[10,"平底锪钻","8-4.5 ","根",14,"材料含铝 501高速钢材料具有较强的抗冲击能力/跟耐磨性，材料硬度HRC 63-68度，可加工不锈钢，模具钢等难加工材料的工件， 沉孔钻刃径8mm*4.5导柱直径。"]
[11,"平底锪钻","10-5.5 ","根",14,"材料含铝 501高速钢材料具有较强的抗冲击能力/跟耐磨性，材料硬度HRC 63-68度，可加工不锈钢，模具钢等难加工材料的工件， 沉孔钻刃径10mm*5.5导柱直径。"]
[12,"90°锥形锪孔钻","1*5","根",14,"用于锪锥形孔，1*5"]
[13,"90°锥形锪孔钻","5*10","根",14,"用于锪锥形孔，5*10"]
[14,"钢字头","字母、数字3mm","根",1,"字母钢印数字直径3mm"]
[15,"机械工人切削手册第8版","机械工业出版社作者厂","本",7,"机械工业出版社\n作者 原北京第一通用机械厂"]
[16,"图解电工快速入门与提高 ","化学工业出版社 作者 蔡杏山","本",7,"化学工业出版社 \n作者 蔡杏山"]
[17,"袖珍式计算器",null,"个",7,"袖珍式"]
[18,"圆柱头内六角螺钉","M4 x 12","根",100,"M4 x 12"]
[19,"垫片",4,"个",100,"4寸"]
[20,"六角螺母","M4","个",100,"M4"]
[21,"一字螺丝刀","3×75mm","把",14,"3×75mm"]
[22,"一字螺丝刀","5×100mm","把",14,"5×100mm"]
[23,"一字螺丝刀","6×150mm","把",14,"6×150mm"]
[24,"十字螺丝刀","3×75mm","把",14,"3×75mm"]
[25,"十字螺丝刀","5×100mm","把",14,"5×100mm"]
[26,"十字螺丝刀","6×150mm","把",14,"6×150mm"]
[27,"仪表螺丝刀",null,"套",14,"拆卸仪表专用套组"]
[28,"斜口钳",null,"把",14,"8\""]
[29,"尖嘴钳",null,"把",14,"8\""]
[30,"钢丝钳",null,"把",14,"8\""]
[31,"剥线钳",null,"把",14,"8\""]
[32,"压线钳","0.14-2.5mm2","把",14,"0.14-2.5mm2"]
[33,"电工刀",null,"把",14,"100*105mm "]
[34,"布剪刀",null,"把",14,"电工专用"]
[35,"活动扳手","8寸","把",14,"8\""]
[36,"电烙铁",null,"把",14,"220V,35W"]
[37,"网孔板","550 x 700 mm","张",10,"550 x 700 mm"]
[38,"定距销","直径20 x 180圆柱头螺钉M5 ","根",100,"直径20 x 180圆柱头螺钉M5 "]
[39,"三色报警灯柱","红绿白","套",10,"预装带导线的M12快插接头，TD50 DC24v 共阴极"]
[40,"电容式接近开关（PNP型）",null,"套",10,"3线接口，1NO，PNP-输出，DC 24V，带M12-1x（≥30）螺纹的金属外壳"]
[41,"感应式接近开关（PNP型）",null,"套",10,"3线接口，1NO，PNP-输出，DC 24V，带M12-1x（≥30）螺纹的金属外壳"]
[42,"8孔M12输入/输出分配器","8个插孔，每插孔2个信号","个",14,"8个插孔，每插孔2个信号，4线+PE,带主电缆"]
[43,"T形分配器","与本表中序号5相配","个",42,"带2个M12快速连接头，Y型M12圆形连接器"]
[44,"PLC","DC 24V/4A;满足24输入24输出","个",7,"DC 24V/4A;满足24输入24输出"]
[45,"配电柜","600x800x≥250mm","台",10,"600x800x≥250mm"]
[46,"直流电源","DC24V/4V","台",10,"DC24V/4V"]
[47,"电器导轨",null,"套",28,"与本表中序号52（端子板）相配"]
[48,"端角",null,"个",84,"与本表中序号52（端子板）相配"]
[49,"盖板","4个灰色，2个蓝色","个",84,"4个灰色，2个蓝色，与本表中序号52（端子板）相配"]
[50,"端子板","2.5mm²，灰色","个",600,"2.5mm²，灰色，与本表中序号49（电器导轨）相配"]
[51,"端子板","2.5mm²，蓝色","个",90,"2.5mm²，蓝色，与本表中序号49（电器导轨）相配"]
[52,"PE端子板","2.5mm2","个",90,"2.5mm2，与本表中序号49（电器导轨）相配"]
[53,"PE端子板","6mm2","个",60,"6mm2，与本表中序号49（电器导轨）相配"]
[54,"标记牌",null,"个",600,"与本表中序号52（端子板）相配"]
[55,"连接桥",null,"个",600,"与本表中序号52（端子板）相配"]
[56,"安全继电器","DC24V,双通道，","个",8,"DC24V,双通道，在输入回路有接地、短路和交叉识别功能，启动受监控，反馈电路用来监控外部的接触器（≥2个NO）"]
[57,"负载隔离开关","3线，25A","个",14,"3线，25A，用于安装/加装IP40"]
[58,"接触器","4kw，DC24V;3H+2NC,2NO","个",42,"4kw，DC24V;3H+2NC,2NO，带灭弧装置"]
[59,"电机保护开关","3×0.11-0.16A(带辅助触点1NC,1NO)","个",14,"3×0.11-0.16A(带辅助触点1NC,1NO)"]
[60,"断路器","B10A,1极","个",14,"B10A,1极"]
[61,"断路器","B6A,1极","个",14,"B6A,1极"]
[62,"断路器","C4A,1极","个",14,"C4A,1极"]
[63,"漏电保护器（RCD）","16A/10mA,2极，A型","个",14,"16A/10mA,2极，A型"]
[64,"CEE三相交流插头","5极，400V,16A,6h","个",14,"5极，400V,16A,6h，用于安装/加装"]
[65,"卡式插座","230V,16A，带保护触点","个",14,"230V,16A，带保护触点，安装在电器导轨上"]
[66,"扩展安装壳","40极插孔组","个",28,"40极插孔组，使用矩形插头20芯代替，两组代替一组"]
[67,"40极插孔组","压接式*/旋接式/非旋接式","个",28,"压接式/旋接式/非旋接式"]
[68,"活插外壳","40极插孔组+PE 1个","个",14,"40极插孔组+PE 1个"]
[69,"40极插孔组","压接式*/旋接式/非旋接式","个",28,"压接式/旋接式/非旋接式"]
[70,"CEE三相交流插头","4极，400V,16A,6h","个",14,"4极，400V,16A,6h，用于安装/加装"]
[71,"布线槽","开槽，至少约 80x80 mm","个",28,"开槽，至少约 80x80 mm"]
[72,"布线槽","开槽，至少约 45x65 mm","个",28,"开槽，至少约 45x65 mm"]
[73,"塑料导线","深蓝色 BVR 0.5mm2（控制电路24V）","根",1400,"深蓝色 BVR 0.5mm2（控制电路24V）"]
[74,"塑料导线","浅蓝色 BVR 1.5mm2（零线）","根",200,"浅蓝色 BVR 1.5mm2（零线）"]
[75,"塑料导线","红色 BVR 1.5mm2（230V）","根",84,"红色 BVR 1.5mm2（230V）"]
[76,"塑料导线","黑色 BVR 1.5mm2（230V）","根",84,"黑色 BVR 1.5mm2（230V）"]
[77,"塑料导线","绿/黄色 BVR 1.5mm2（保护线）","根",100,"绿/黄色 BVR 1.5mm2（保护线）"]
[78,"塑料导线","紫色 BVR 1.5mm2（急停开关装置）","根",200,"紫色 BVR 1.5mm2（急停开关装置）"]
[79,"塑料导线","黑色 BVR 2.5mm2（主电路）","根",200,"黑色 BVR 2.5mm2（主电路）"]
[80,"塑料导线","橙色 BVR 2.5mm2（保护线）","根",200,"橙色 BVR 2.5mm2（保护线）"]
[81,"塑料导线","绿/黄色 BVR 6mm2（保护线）","根",200,"绿/黄色 BVR 6mm2（保护线）"]
[82,"冷压端子","带绝缘","个",100,"带绝缘"]
[83,"环形线鼻子","带绝缘","个",100,"带绝缘"]
[84,"尼龙扎带","100 mm","根",400,"100 mm"]
[85,"尼龙扎带固定座",null,"个",200,"固定扎带"]
[86,"操作面板","18个安装孔位","个",14,"18个安装孔位"]
[87,"急停开关（嵌入式）","双通道，2NC，带自锁功能","个",14,"双通道，2NC，带自锁功能，与本表中序号88（操作面板）相配"]
[88,"旋钮开关（嵌入式）","1NO,0-1，带自锁功能","个",28,"1NO,0-1，带自锁功能，与本表中序号88（操作面板）相配"]
[89,"带灯按钮（嵌入式）","1NO，24V,红色","个",14,"1NO，24V,红色，与本表中序号88（操作面板）相配"]
[90,"带灯按钮（嵌入式）","1NO，24V,白色","个",14,"1NO，24V,白色，与本表中序号88（操作面板）相配"]
[91,"指示灯（嵌入式）","白色6个，绿色1个","个",84,"白色6个，绿色1个，与本表中序号88（操作面板）相配"]
[92,"安装位置堵头",null,"个",140,"与本表中序号88（操作面板）相配"]
[93,"软控制线",null,"根",50,"0.75mm2，40极+PE,去除张力"]
[94,"自粘标签",null,"张",10,"用于标注部件"]
[95,"焊锡丝",null,"盘",2,"焊接专用"]
[96,"线号",null,"根",60,"与导线相匹配"]
[97,"单出杆双作用带磁环气缸","φ10×40　　　　　","套",14,"φ10×40；活塞杆头为螺纹型并配锁紧螺母　，配2个缸用单向节流阀（排气节流）"]
[98,"5/3双作用电磁换向阀","DN4～6mm，","个",14,"通径DN4～6mm，DC24V，1m预装线，先导型(可手动换向),中位“O”型，配气管快插接头和消声器;预装M12快插接头"]
[99,"阀座","带手动辅助换向","个",14,"带手动辅助换向，配气管快插接头和消声器；"]
[100,"3/2单作用电磁换向阀","带手动辅助换向","个",14,"带手动辅助换向，配气管快插接头和消声器；预装M12快插接头"]
[101,"压力开关","DC24V","个",14,"1-6巴，DC24V, 1个转换点或1NO-1NC (也可以是电子三线压力传感器)，含M12快插接头，与第5相配，压力开关管径与气管配，带支架"]
[102,"带表减压阀","1～8巴","个",14,"1～8巴，配气管快插接头（90°可转），带支架"]
[103,"磁性接近开关","DC 24V","个",28,"DC 24V，通过磁环启动，带连接导线，1 NO，3线接口，含M12快插接头"]
[104,"金属扎带",null,"根",28,"固定磁性开关用，与气缸相配"]
[105,"T型快插接头（三通）",null,"个",28,"与气管直径相配"]
[106,"塑胶管","外径4mm或6mm","根",28,"外径4mm与元件快插接头相配"]
[107,"塑料扎带","100mm","根",800,"100mm"]
[108,"生胶带",null,"卷",10,"密封专用"]
[109,"螺丝、螺母",null,"套",200,"按照各器件固定孔配螺钉螺母（套装）"]
[110,"快走丝线切割钼丝","Φ0.18","卷",2,"Φ0.18"]
[111,"* 机械设计软件","中望机械设计软件V2014\n\n*提供原厂授权和售后服务承诺","点",30,"\n\n内核\n软件采用自主研发的全新内核，采用独创的内存管理机制和高效的运算逻辑技术，针对双核\nCPU及多线程机制优化算法能够适应更复杂的图形文件，并且在相同条件下软件的\n运行也更流畅。\n文件兼容\n软件采用DWG为内部工作文件格式，能够读取和保存DWG、DXF文件，高度兼容AutoCAD 2.5~2012\n版所有图形文件，读取和存储图形信息完整准确。\n手势精灵\n用户使用鼠标进行简单或按设定的轨迹移动，即可执行相应的绘图命令。\n手势精灵定制\n用户可以自定义鼠标手势的设置，满足个性化的需求，提升绘图效率。\n工具选项板\n工具选项板以选项卡形式来组织、共享和放置命令、块及其它工具，具备机械、建筑、\n电子方面的实用图块，拖拽即可使用，用户也可自定义图块放入工具选项版中使用。\n文字\n文字解析统一使用UNICODE编码，文字显示正确性高，支持单行文字和多行文字，编辑文字时能够实时显示文字的样式和大小状态。同时，软件拥有15个语言版本，包含中文简体、中文繁体、英文、法文、日文、西班牙文、葡萄牙文等等，方便CAD图形文件跨国交流。\n修订云线\n修订云线功能支持手绘样式，并可以将圆弧、直线、多段线或样条曲线转换为云线。\n标注关联\n标注增加关联性，在对图形对象进行修改的同时，标注对象也随之更改，以符合更改后的图形，修改图形的工作量相应减少。\n支持OLE对象\n软件能够插入OLE对象，如office软件的内容复制后可直接粘贴到软件的图形中，软件的图形也可以直接粘贴到office\n中。双击OLE对象，即可启动对象对应的程序来进行修改。\nRibbon界面\nRibbon界面是将图标更加合理的分组，极大的减少了面板的展开界面，优化了操作步骤，使应用程序的功能更加易于发现和使用。\n块属性管理器\n用于管理当前图纸中所有块里包含的属性，可以方便地进行批量修改块属性的各项属性，并通过对话框中的“同步”按钮，使其同步更新。\n智能定义属性\n除了基本的属性定义功能以外，还可对属性定义进行多行文字的插入，并支持文字字高的点选支持，旋转角度的点选，除此以外可以在属性信息中插入字段。\n多视口显示\n在一张图纸中无缝的多视口显示图形，且视口的观察角度和视觉样式都可以独立设置，该功能在三维设计时更为方便，使图纸编辑、比对更快速更高效。\n布局视口最大化\n在布局空间工作时，它会将当前视口最大化，便于编辑修改，并可自由Pan/Zoom；完成后使用VPMIN功能，恢复视口和布局显示，此时在视口将自动恢复到放大前的范围和比例，无需手动调节。\n电子传递\n可以对图纸文件进行打包，且包中的图形文件会自动包含所有相关的文件，如外部参照和字体文件，解决了在图纸交流情况下因为缺少特定的文件而造成的无法使用图形文件的问题。\n格式刷跨图纸操作\n特性匹配支持跨图纸操作，用户可以从旧图纸中复制属性匹配到新图纸的对象中，便于图纸格式统一，资源重复利用。\n图层转换器\n可以将cad图层进行批量的转换、合并\n文档图像预览\n可将最近打开的九个文档进行大图像预览"]
[112,"* 数控铣床","XD-40A(数控系统华中世纪星HNC-22M）\n\n*提供原厂授权和售后服务承诺","台",1,"1、机床底座、立柱、主轴箱体、十字滑台、工作台等基础件全部采用高强度铸造成型技术，内部金相组织稳定，确保基础件的高稳定性。铸件结构经过机床动力学分析和有限元3分析，使其几何结构更加合理，与加强筋的恰当搭配，保证了基础件的高刚性。宽实的机床底座，箱形腔立柱、加宽加长的床鞍、负荷全支撑的设计，结构符合材料力学的先进设计理念，可确保加工时的重负载能力。\n2、高速、高精密主轴：\n(1)主轴电机通过高扭力齿形皮带传动，不打滑，并可大幅减低传动噪音及热量产生。\n(2)主轴采用精密级斜角滚珠轴承和滚柱轴承，高速高精密，标准转速可达8000r/min。\n(3)高性能油脂润滑主轴轴承，经济的主轴头冷却系统，有效地控制主轴高速温升。\n(4)主轴利用IRD动态平衡较正设备，直接校正主轴动态平衡，使主轴在高速运转时，避免产生共振现象，确保最佳的加工精度。\n3、X、Y、Z轴进给均采用直线滚动导轨支撑，配之高精度滚珠丝杠副，滚珠丝杠经预拉伸后，大大增加了传动刚度并消除了快速运动时产生的热变形影响，因而确保了机床的定位精度和重复定位精度。主轴箱移动（Z轴）配有中央导引设计的平衡锤装置，华中数控系统系统，即使在高速移动时，配重也不产生晃动。配重与主轴箱重量比例精确可获得最佳的加工特性。且使Z轴驱动电机具有良好的负载特性。\n4、机床配有密封式导轨防护罩，有效的保护导轨和丝杠，延长其使用寿命。\n5、当机床选配全防护时，可应用螺旋式自动排屑装置。该装置简洁、环保，适用于金属和非金属切屑的输送。（对于铸铁屑、铝卷屑和铁卷屑，建议选配链板式或刮板式等其它排屑装置）。机床配以手动喷（水）枪（选配），易于清除铁屑。\n6、CNC控制系统采用标准配置FANUC-0i数控系统。大连系统可选。数控系统可配备四轴接口，工件/刀具测量接口，标准RS-232接口及DNC功能。\n7、高效率自动润滑系统：导轨润滑采用容积分配器搭配注油，定量供给导轨所需用油，减少润滑油的浪费，避免环境污染。\n8、精巧的油水分离设备：机床设计时，考虑油水分离的需求，润滑轨道的废油集中到底座后方油水分离箱，减少切削液油水的混合，避免切削液变质，延长使用寿命。\n9、电气柜内的配线皆符合国家电气安全规范，确保控制系统运转时不受外部干扰。采用热交换器，使电气箱内的热空气迅速排出，保持箱内的恒温，使控制系统能长期稳定的运转。同时有更高安全要求的客户可以选择符合“CE”认证的产品，采用双通道的安全模式，更好的保证生产安全。\n10、高精度螺距补偿，各传动轴均采用高精度激光测量仪补偿使各轴定位精度更加准确，更适合加工高精度的零件。"]
[113,"* 气动与PLC实训装置","天煌THPQD-1型\n\n*提供原厂授权和售后服务承诺","台",1,"技术参数 \n1. 输入电源： 三相五线 380V±10% 50Hz\n2. 系统压力： ≤6. 3MPa \n3. 变量叶片泵： 压力调节范围 4MPa～7MPa； 额定流量 8L/min(1800rpm) \n4. 电机： 额定电压 380V， 额定功率 1. 5kW， 绝缘 B \n5. PLC： 采用德国西门子 S7-200 系列， CPU224 输入 14 点/输出 10 点（继电器型） \n6. PCI-1711 数据采集卡： PCI-1711 是一款功能强大的多功能 PCI 总线数据采集卡， 有 16路单端模拟量输入/2 路模拟量输出； 16 路数字量输入及 16 路数字量输出； 12 位 A/D 转换器， 采样速率可达 100kHz \n7. 安全保护： 具有漏电压、 漏电流、 过载、 接地、 缺相及相序保护装置， 安全符合国家标准。"]
[114,"* 锯床","GD4038半卧式金属带锯床\n\n*提供原厂授权和售后服务承诺","台",1,"1、切削范围：圆料：380mm 板材：400mm\n2、带锯条规格：4115*34*1.1mm\n3、给进速度：液压无级调速\n4、主电机功率：3kw,3级（20/40/60）\n5、液压电机功率：0.55kw\n6、机床尺寸：2300*1150*1500mm（长*高*宽）\n"]
[115,"机械制图挂图","高等教育出版社 ISBN：9787040234817","套",1,"高等教育出版社 ISBN：9787040234817"]
[116,"14寸耐用工具箱","九鼎","个",10,"0.8mm冷扎钢板和全新工程塑料规格：14寸 长度为：450MM"]
[117,"电焊机","ZX7-200KE(220V)带防护罩","台",1,"输入电压(V)220\n额定输入容量(KVA)7.1\n输出空载电压(V)62\n电流调节范围(A)20-160\n焊接电流负载持续率60%(A)160\n负载持续率100%(A)124\n重量(KG)7\n外形包装尺寸：LxWxH(mm)470x270x345\n焊机代码0.29.017-6-1\n母材材质 碳钢  低合金钢  不锈钢\n板厚(mm)2.0-6.0\n焊条直径(mm)1.6-4.0 "]
[118,"硬质合金立铣刀","∮6","支",40,"∮6"]
[119,"硬质合金立铣刀","∮10","支",40,"∮10"]
[120,"硬质合金立铣刀","∮8","支",40,"∮8"]
[121,"硬质合金立铣刀","∮16","支",40,"∮16"]
[122,"硬质合金立铣刀","∮4","支",40,"∮4"]
[123,"硬质合金立铣刀","R4","支",40,"R4"]
[124,"硬质合金立铣刀","R2","支",40,"R2"]